**K A S S U J O I N T E X A M I N A T I O N**

**SEPTEMBER 2021**

**441/2**

**HOME SCIENCE**

**CLOTHING AND CONSTRUCTION**

**PAPER 2**

**MARKING SCHEME**

**Name: ……………………………………………………….....................................Index No.: ………………**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  | **TASKS** | **MAX. SCORE** | **ACTUAL SCORE** | **REMARKS** |
| **1.** |  | **PRESENTATION** |  |  |  |
|  | (a) | Work well pressed and well folded | 1 |  |  |
|  | (b) | Label stitched on a single fabric | 1 |  |  |
|  | (c) | Clearly written Name, Adm. No., Class | 1 ½ |  |  |
|  | (d) | Pins, unnecessaary tacking and hanging threads removed | 1 ½ |  |  |
|  | (e) | Made up left half | 1 |  |  |
|  |  | **SUB TOTAL** | **6** |  |  |
| **2.** |  | **CUTTING OUT** |  |  |  |
|  | (a) | All the 10 pieces cut out. | 5 |  |  |
|  | (b) | Smooth cuttting of the front skirt and on the striaght grain on CF | 2 |  |  |
|  | (C) | Smooth cutting of the front yoke and on straight grain at the CF | 2 |  |  |
|  | (d) | Smooth cutting of the skirt back on straight grain at the CB. | 2 |  |  |
|  | (e) | Smooth cutting of the front frill and on staight grain at CF | 2 |  |  |
|  | (f) | Smooth cutting of the back frill and on straight grain at the CB. | 2 |  |  |
|  | (g) | Smooth cutting of the waistband and on straight grain at the CF | 3 |  |  |
|  |  | **SUB TOTAL** | **18** |  |  |
| **3.** |  | **BACK DART** |  |  |  |
|  | (a) | Straight and firm stitchery of the dart | 1 |  |  |
|  | (b) | Tapering to nothing and not forming pockets | 1 |  |  |
|  | (c) | Correct size of the dart (8cm) and width (2cm) to within 2mm | 1 |  |  |
|  | (d) | Well fastened at the tip | 1 |  |  |
|  | (e) | Well pressed and towards the CB | 1 |  |  |
|  |  | **SUB TOTAL** | **5** |  |  |
| 4 |  | **JOINING THE FRONT YOKE TO FRONT SKIRT (overlaiad seam if not give zero)** |  |  |  |
|  | (a) | Overlay yoke folded to the W.S at the stitching line. | 1 |  |  |
|  | (b) | Overlay placed on the underlay (skirt) stitching line on the R.S | 1 |  |  |
|  | (C) | Seam stitched with straight and firm stitchery and close to the folded on the R.S. | 11/2 |  |  |
|  | (d) | Seam turnings trimmed to 1cm and neatened together. | 1 |  |  |
|  | (e) | Appropriate neatening stitches use. *(If not neatened give zero from g –j)* | 1 |  |  |
|  | (f) | Eveness of the stitches | 1 |  |  |
|  | (g) | Correct tension of the stitches | 1 |  |  |
|  | (h) | Neat stitches | 1 |  |  |
|  | (i) | Fastened on and off | 1 |  |  |
|  | (j) | Seam well pressed and flat | 1 |  |  |
|  |  | **SUB TOTAL** | **101/2** |  |  |
| 5 |  | **ATTACHING THE IN SEAM POCKET** |  |  |  |
|  | (a) | The pockets attached to the back and front skirt using firm and straight stitchery. | 2 |  |  |
|  | (b) | The pocket attached with smooth and firm stitchery | 1 |  |  |
|  | (c) | Raw edges trimmed and neatened appropriately | 1 |  |  |
|  | (d) | Correct size and shape of the pocket | 1 |  |  |
|  | (e) | Correct positioning of the pocket | 1 |  |  |
|  | (f) | Mouth pocket reinforced on the R.S | 1 |  |  |
|  |  | **SUB TOTAL** | **7** |  |  |
| **6.** |  | **SIDE SEAM *(*Open seam, if not give zero)** |  |  |  |
|  | (a) | Seam done with firm and straight stitchery. | 1 |  |  |
|  | (b) | Seam turnings neatened separately and appropriately. | 1 ½ |  |  |
|  | (c) | Correct size of the neatened turnings (1cm to within 2mm) | 1 |  |  |
|  | (d). | Evenness of the neatened turnings. | 1 |  |  |
|  | (e) | Seam pressed open and flat at the hem | 2 |  |  |
|  |  | **SUB TOTAL** | **6 ½** |  |  |
| **7.** |  | **JOINING FRONT AND BACK FRILLS (Double stitched)** |  |  |  |
|  | (a) | Front and back facing joined with straight and firm stitchery of the 1st line. | 1 |  |  |
|  | (b) | Firm and straight stitchery of the 2nd line of stitching and close to the fold | 1 |  |  |
|  | (c) | Fell on the back of the work | 1 |  |  |
|  | (d) | Fell folded in to completely conceal the raw edges | 1 |  |  |
|  | (e) | Correct size of the seam | 1 |  |  |
|  | (f) | Evenness of the seam | 1 |  |  |
|  | (g) | Flat on the right and wrong side | 1 |  |  |
|  |  | **SUB TOTAL** | **7** |  |  |
| **8.** |  | **JOINING THE LOWER SKIRT TO THE JOINED FRILL (plain seam if not give zero)** |  |  |  |
|  | (a) | Firm and straight stitchery | 1 |  |  |
|  | (b) | Seam turnings trimmed to 1cm | 1 |  |  |
|  | (c) | Seam turnings neatened together | 1 |  |  |
|  | (d) | Appropriate stitches used if stitches not appropriate give zero from (d) to (f) | 1/2 |  |  |
|  | (e) | Good tension and evenness of the stitches | 1 |  |  |
|  | (f) | Stitches neatly done and reinforced on and off | 11/2 |  |  |
|  |  | Well pressed & flat complete seam | 1 |  |  |
|  |  | **SUB TOTAL** | **7** |  |  |
| **9.** |  | **WAISTBAND (INTERFACED)** |  |  |  |
|  | **A** | **PREPARATION** |  |  |  |
|  | (a) | Waist band joined with firm and straight stitchery | 1 |  |  |
|  | (b) | Seam trimmed to 0.5cm | 1 |  |  |
|  | (c) | Waistband well knife edged | 1 |  |  |
|  | (d) | Waist band interfaced | 1 |  |  |
|  |  | **SUB TOTAL** | 4 |  |  |
|  | B | **ATTACHMENT** |  |  |  |
|  | (a) | Back waist band joined to back skirt and the vice versa | 2 |  |  |
|  | (b) | Waist band joined to skirt with firm and straight stitchery | 1 |  |  |
|  | (c) | Seam turnings trimmed to 0.5cm | 1 |  |  |
|  | (d) | Waistband neatened using hemming stitches (if hemming stitches are not used give zero from (d) to (f) | 1 |  |  |
|  | (e) | Correct tension and evenness of the stitches | 1 |  |  |
|  | (g) | Stitches neatly done and reinforced on and off. | 1 |  |  |
|  | (h) | Correct size of the finished waistband to within 0.2cm | 1 |  |  |
|  | (i) | Waist band flat on W.S and R.S | 1 |  |  |
|  |  | **SUB TOTAL** | **9** |  |  |
| **10.** |  | **BUTTON HOLE** |  |  |  |
|  | (a) | Button hole worked with by hand worked button hole stitches and not loop stitches. If not buttonhole stitches give zero from (a) to (f) | 1 |  |  |
|  | (b) | Correct tension and size of the stitches | 1 |  |  |
|  | (c) | Neatly and evenly worked | 1 |  |  |
|  | (d) | Straining end of buttonhole rounded and the other end squared | 1 |  |  |
|  | (e) | Stitches on bottom and top of buttonhole | 2 |  |  |
|  | (f) | Stitches reinforced on and off. | 1 |  |  |
|  | (g) | Correct size and position of the button hole | 2 |  |  |
|  | (h) | General impression of button hole. | 1 |  |  |
|  |  | **SUB TOTAL** | **10** |  |  |
|  |  | **GRAND TOTAL** | **X/90** |  |  |