232/1

PHYSICS

PAPER 1

MARKING SCHEME

1. Diameter of wire = 1.33

Radius of wire 1.33÷2🗸1=0.67cm🗸1

1. To increase the time take to come to a stop which reduces the rate of change of momentum or reducing the impulsive force producing a small reaction on him by floor🗸1
2. Clean water has a high surface tension addition of detergent lowers the surface tension 🗸1
3. Mlf+mcΔT🗸1=

 =16800+1050

 =17850J🗸1

1. A1V1=A2V2🗸1

π=πx20x🗸1

V2=🗸1

1. Pressure is developed at the point of application of the force. 🗸1Since the liquid is incompressible, pressure is uniformly transmitted and force is generated.🗸1
2. Hydraulic machines (brakes, press)🗸1
3. F=

 V=4.00m/s🗸1

1. E=4.25-4.00=0.25m

F=Ke= >75=0.25k🗸1

K=300N/M🗸1

1. The level of water in the tube first drops and then rises. 🗸1Due to expansion of the glass boiling tube.🗸1
2. The c.o.g is raised when the carrier is at the top lowering the stability.🗸1
3. Copper a good conductor of heat conducts the heat away hence paper does not char.🗸1
4. Wx5=4x20√

W=√



√1

1. The temperature at which the volume pressure/K.E of a gas is assumed to be zero.🗸1
2. Halving the volume doubles the number of collisions per unit time.🗸1Therefore the rate of change of momentum will also double.🗸2
3. I -Serves as a pointer to the volume on scale

-A drying agent for the gas🗸1

II -To make the temperature of the bath uniform.🗸1

1. Heat the bath and record the temperature and height at suitable temperature interval.🗸1 plot a graph of volume against temperature.🗸1 The graph is a straight line indicating proportional change in volume and temperature.
2. See sketch on grid.
3. P1V1=P2V2🗸1

X=🗸1

1. Introduce the oil drop on the water surface.🗸1The surface tension of water reduces and the net force🗸1 of the surrounding water pulls oil molecules outwards hence spreading.🗸1
2. Ah=volume🗸1

2

 ππ🗸1

h=🗸2

1. Oil patch is a perfect circle, a monolayer🗸1

Oil drop is perfect sphere🗸1

1. To make boundary of oil patch visible🗸1
2. Trapping oil in a loop of wire and holding it against a mm scale.🗸1View the oil drop under a magnifying lens (glass) to enable correctly measure diameter.🗸1

 u =

1. v
2. a
3. i) h🗸1

 45= 🗸1 or u=

 T=3sec 🗸1 = 30m/s🗸1

 V = u-gt🗸1

 O = 30-10t, 🗸1t=3sec🗸1

1. T =2t s = vt

=2(3) = 50x6√1

=6sec🗸1 = 300m√1

1. a )
2. V.R🗸1

 =

 But sinθ==V.R=🗸1

1. η=🗸1

 65= x 100 √1

 65=

MA=1.3🗸1

1. Energy is lost as friction force on the inclined surface🗸1
2. V.R=4
3. M.A increases as the load increases
4. P.E K.E heat+sound
5. a)

This is the quantity of heat required to raise the temperature of unit mass of substance by one kelvin.🗸1

1. Some of the heat is used to warm the insulating cover and surrounding area.🗸1
2. The heater was still hot (at a higher temperature than the block/continues heating cooling.🗸1
3. Power supplied= IV=10x22=220W🗸1

Slope=

Pt=McΔθ

M=2kg

C=

1. Heat lost to the surrounding,🗸1 heat used to warm up the insulating cover and thermometer🗸1 or heat is lost to warm insulating cover and thermometer.🗸🗸

1000

 500

 00

2400

 X0

400

= √1

 = √1

 = 1400√1

18.C