**441/2**

**HOME SCIENCE**

**JULY, 2019**

**PAPER 2**

**(Clothing Construction)**

**Marking scheme**

**BUURI EAST STANDARDS**

***Kenya Certificate of Secondary Education***

**HOME SCIENCE 441/2**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **PROCESSES** | **MAX SCORE** | **ACTUAL SCORE** | **REMARKS** |
| 1 | **PRESENTATION** |  |  |  |
|  | Work well pressed (1) and well folded (1) | 2 |  |  |
|  | Label firmly fixed,(1) without concealing details (1) and on a single fabric (1) | 3 |  |  |
|  | Pins ( ½ ) tacking threads ( ½ ) and unnecessary threads ( ½ ) removed | 1 ½ |  |  |
|  | Made up for the right half ( 1) | 1 |  |  |
|  | **Sub total** | **7 ½** |  |  |
| **2** | **CUTTING OUT** |  |  |  |
|  | All six pieces cut out ( 6 x ½ ) | 3 |  |  |
|  | Smooth cutting on blouse at C F ( 1) | 1 |  |  |
|  | Smooth cutting on blouse at C B ( 1) | 1 |  |  |
|  | Straight grain on blouse at C B ( 1) | 1 |  |  |
|  | Smooth cutting of yoke at CB ( 1) | 1 |  |  |
|  | Straight cutting of back facing at CB (1) | 1 |  |  |
|  | Straight grain on back facing at CB ( 1) | 1 |  |  |
|  | Straight cutting of collar and interfacing ( 3 x 1) | 3 |  |  |
|  | Straight grain of the collar and interfacing 2 x 1 = 2 | 2 |  |  |
|  | Smooth cutting of the lower edge ( 1) | 1 |  |  |
|  | **Sub total** | **15** |  |  |
| 3 | **WORKING OF THE BUST DART** |  |  |  |
|  | Made with straight stitchery ( 1) | 1 |  |  |
|  | Tapering to a point ( 1) | 1 |  |  |
|  | Threads well secured (1) | 1 |  |  |
|  | Correct length ( 9cm) ( 1) | 1 |  |  |
|  | Correct width 0.9mm to within 2mm | 1 |  |  |
|  | Dart pressed down wards ( 1) | 1 |  |  |
|  | Dart flat on RS ( ½ ) and WS ( ½ ) | 1 |  |  |
|  | **Sub total** | **7** |  |  |
| **4** | **INVERTED PLEAT** |  |  |  |
|  | ( If not inverted on the R.S, award zero mark (0) |  |  |  |
|  | Folding of pleat along the fold line | 1 |  |  |
|  | Correct depth of pleat to within 2mm | 1 |  |  |
|  | Correct width of pleat to within | 1 |  |  |
|  | Top stitching done above and below | 1 |  |  |
|  | Folds meet at the centre on a foldline | 1 |  |  |
|  | **Sub total** | **5** |  |  |
| **5** | **PREPARATION AND JOINING THE YOKE** |  |  |  |
|  | Joined with an overlaid seam, (if not overlaid award zero mark) | 2 |  |  |
|  | Seam made with smooth stitchery | 1 |  |  |
|  | Stitches close to the edge to within 2mm | 1 |  |  |
|  | Yoke mitred ( ½ ) and flat on top of the pleat ( ½ ) | 1 |  |  |
|  | Raw edges trimmed ( 1) and neatened with loop stitches ( 1) |  |  |  |
|  | Correct tension of loop stitches | 2 |  |  |
|  | Evenly spaced loop stitches | ½ |  |  |
|  | Even length of loop stitches | ½ |  |  |
|  | Correct size of the seam 1cm to within 2mm (0.8 – 1.2cm) | ½ |  |  |
| j | Correct shape of attached yoke, superimpose to within 5mm | ½ |  |  |
|  | **Sub – total** | **9 ½** |  |  |
| 6 | **MAKING MACHINE FELL SEAM AT THE SHOULDER** |  |  |  |
|  | If not machine fell seam award zero | 2 |  |  |
|  | Straight stitching on first row | 1 |  |  |
|  | Straight stitching on second row | 1 |  |  |
|  | Stitching close to the folded edge | 1 |  |  |
|  | Even width | 1 |  |  |
|  | Correct size 0.6 to within 2mm ( 0.4 – 0.8mm) | 1 |  |  |
|  | Fell neatly tucked under | 1 |  |  |
|  | Flatness of seam RS ( 1) and WS (1) | 2 |  |  |
|  | Seam worked on RS | 1 |  |  |
|  | Fell pressed towards the back | 1 |  |  |
|  | **Sub – total** | **12** |  |  |
| 7 | **MAKING OF FRENCH SEAM AT THE SIDE** |  |  |  |
|  | **If not French seam, award zero makrs ( 0)** | **2** |  |  |
|  | Seam joined with straight stitches | 1 |  |  |
|  | Raw edges well concealed and no threads on the RS (1) | 1 |  |  |
|  | Good knife – edge | 1 |  |  |
|  | Even width | 1 |  |  |
|  | Correct size 0.6 to within 2mm ( 0.4 – 0.8) | 1 |  |  |
|  | Seam pressed towards back | 1 |  |  |
|  | **Sub – total** | **8** |  |  |
| 8 | **JOINING OF FRONT & BACK FACINGS** |  |  |  |
|  | Back and front facing correctly joined (1) with straight ( ½ ) and even ( ½ ) stitchery | 2 |  |  |
|  | Seam trimmed ( ½ ) and unneatened ( ½ ) | 1 |  |  |
|  | Seam pressed open ( 1) | 1 |  |  |
|  | **Sub – total** | **4** |  |  |
| **9** | **NEATENING OF BLOUSE FRONT FACING** |  |  |  |
|  | Appropriately neatened | 1 |  |  |
|  | Straight stitches | 1 |  |  |
|  | Even stitches | 1 |  |  |
|  | Stitches close to the fold | 1 |  |  |
|  | **Sub – total** | **4** |  |  |
| 10 | **COLLAR PREPARATION** |  |  |  |
|  | Smooth stitchery ( 1) of outer edge of collar ( mark by impression. | 1 |  |  |
|  | Collar seam trimmed | ½ |  |  |
|  | Good knife edge | ½ |  |  |
|  | Collar interfaced ( 1) at the undercollar (1) | 2 |  |  |
|  | **Sub – total** | **4** |  |  |
| 11 | **COLLAR ATTACHMENT** |  |  |  |
|  | Correctly positioned from fold line (1) and flash at CB ( 1) to within 2mm | 2 |  |  |
|  | Collar sandwiched between facing and garment (1) | 1 |  |  |
|  | Neckline trimmed ( ½ ) and snipped ( ½ ) | 1 |  |  |
|  | Smooth attaching line | 1 |  |  |
|  | Correct shape ( 1) and size ( 1) within 5mm (super impoce) | 2 |  |  |
|  | Collar flat | 1 |  |  |
|  | **Sub – total** | **8** |  |  |
| 12 | **BUTTON HOLE** |  |  |  |
|  | Button hole cut on straight grain | 1 |  |  |
|  | Neatened with button hole stitches. If not button hole stitches award zero mark from ( b) to (e) | 1 |  |  |
|  | Even length of stitches | 1 |  |  |
|  | Correct tension | 1 |  |  |
|  | Stitches evenly spaced | 1 |  |  |
|  | Correct size of completed botton hole | 1 |  |  |
|  | **Sub – total** | **6** |  |  |
|  | **TOTAL SCORE** | **90/ 2 = 45** |  |  |

**<<< E N D >>>**