441/2

CLOTHING CONSTRUCTION

MARKING SCHEME

|  |  |  |  |
| --- | --- | --- | --- |
|  | Max score | Actual score | remarks |
| 1. **Presentation**
* Work well pressed(1) and folded(1/2)
* Label firmly fixed (1) without concealing details (1/2 ) and on single fabric(1/2)
* Pins/needles (1/2) tacking threads(1/2) and unnecessary threads (1/2) removed
* Make up for the right half (1)
 | 1 ½ 2 ½ 1 ½ 1 |  |  |
|  | **6 ½** |  |  |
| 1. **Cutting out**
* All five pieces cut out (5x1/2)
* Smooth cutting of front bodice(1)
* Smooth cutting of back bodice (1) and cut on straight grain(1)
* Smooth cutting of back yoke(1) and cut on straight grain(1)
* Smooth cutting of collar(1) and cut on straight grain(1)
* Smooth cutting of back neck facing(1/2) cut on straight grain(1/2)
 | 2 ½ 12221 |  |  |
|  | **10 ½**  |  |  |
| 1. **Making up**
2. Bust dart
* Correct length to within 2mm(1)
* Correct width to within 2mm(1)
* Tapering to a point (1)
* Straight stitchery(1)
* Threads secured (1)
* Flat dart on R.S(1/2) and W.S(1/2)
 | 111111 |  |  |
|  | **6** |  |  |
| 1. **Preparation of gathers**
* Two rows of gathering stitches above (1) and below (1/2) S.L
* Gathers evenly distributed (2)
* Gathering stitches not removed (1/2 x 2)
 | **2****2****1** |  |  |
|  | **5** |  |  |
| 1. **Attachment on the back yoke**

N.B If not overlaid seam give zero.Overlaid seam* Yoke folded on seam line (1)
* Placed on F.L of the back bodice (1)
* Straight stitchery (1) on the edge of the fold (1)
* Overlaid turning facing upwards (1)
* Even seam (1)
* Flat yoke on the R.S (1)
* Not neatened (1/2) not trimmed (1/2)
* Matching notches (1/2) and edges (1/2)
* Seam allowance 1.5cm from fitting line (1) to within 2mm.
* Yokes CB and back bodice CB in flash (1)
 | **1****1****1****1****1****1****1****1****1** |  |  |
|  | **11** |  |  |
| 1. **Machine fell seam**

NB If not machine fell give zero.* Straight stitchery of 1st row (1)
* Fell well tucked under (1) and held down with straight stitchery (1)
* Stitched close to the edge (1)
* Even seam
* Correct size (1) (0.4 – 0.8)
* Flat seam on R.S (1)
* Fell fixed towards the back of shoulder (1)
* Thread secured (1)
 | **1****2****1****1****1****1****1****1** |  |  |
|  | **10** |  |  |
| 1. **Working of an open seam**

NB If not open seam give zero.* Joining with straight stitchery (1)
* Threads well secured (1)
* Appropriate neatening (1/2 x 2)
* Even seam (1)
* Correct width 1cm on either side (1/2 x 2)
* Seam opened (1)
* Flat (1/2) and pressed (1/2)
 | **1****1****1****1****1****1****1** |  |  |
|  | **7** |  |  |
| 1. **Joining back and front facing**
* Correctly joined (1/2 x 2) with straight stitchery (1/2 x 2)
* Free edge of facing correctly edge stitched (2)
* Even (1) edge throughout
* Flat seam (1)
* Seam allowance trimmed (1) and pressed (1/2) open (1/2)
 | **2****2****1****1****2** |  |  |
|  | **7** |  |  |
| 1. **Preparation and attaching of collar**
* Correctly prepared (1)
* Round (1) smooth (1) edges
* Flat colour (1)
* Correctly shaped (1) and size (1)
* Correctly stitched (1) and attached
* Correctly attached (1) and positioned (1)
* Correctly neatened (1) with facing (1)
* Facing lying flat (1)
* Clipped seam (1) allowance
 | **1****2****1****2****1****2****2****1****1** |  |  |
|  | **13** |  |  |
| 1. **Understitching the facing**
* Correct understitching (1)
* Stitches not seen on R.S (1)
* Flat facing (1)
* Seam allowance (1)
* Threads secured (1)
 | **1****1****1****1****1** |  |  |
|  | **5** |  |  |
| 1. **Button hole**

NB if not button hole stitches award zero* Correct positioning (1/2) and the length (1/2) of button hole
* Button hole cut on straight grain (1) and worked with single thread (1)
* Button hole stitches even (1/2) well distributed (1)
* Round end worked with well distributed (1/2) overcastting (1/2) stitches
* Square and complete with bar (1) worked with even (1/2) button hole stitches.
* Row edges concealed by buttonhole stitches (1/2 x 2)
 | **1****1****1****1 ½** **1****1 ½****1** |  |  |
|  | **8** |  |  |
|  | **90** |  |  |