**441/2**

**HOME SCIENCE**

**(CLOTHING CONSTRUCTION)**

**PAPER 2**

**JUNE, 2018**

**KASSU J O I N T E V A L U A T I O N E X A M I N A T I O N S**

**K.C.S.E TRIAL EXAMINATION**

**441/2**

**HOME SCIENCE**

**CLOTHING AND CONSTRUCTION**

**PAPER 2**

**MARKING SCHEME**

**Candidates Name: …………………………………………………………………………..**

**Index No.: ………………………………………**

**Subject Teacher’s Name: …………………………………………………………………**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **1.** | **PRESENTATION** | **MAX. SCORE** | **ACTUAL SCORE** | **REMARKS** |
|  | 1. Work well pressed and folded 2. Label clearly written, firmly fixed on a single fabric without concealing details 3. Unnecessary hanging threads, tacking and pins removed 4. Made up the right half | 1  2  11/2  1 |  |  |
|  | **Sub Total** | **51/2** |  |  |
| **2.** | **CUTTING OUT AND GRAINING** |  |  |  |
|  | 1. All eight pieces cut out 2. Smooth cutting of the back blouse and on straight grain at the centre back. 3. Smooth cutting of the back neck facing and on straight grain at the centre back 4. Smooth cutting of the collar and under collar on straight grain at the centre back | 4  2  2  4 |  |  |
|  | **Sub Total** | **12** |  |  |
| **3.** | **DOUBLE POINTED DART** |  |  |  |
|  | 1. Straight & firm stitchery 2. Tapering to nothing on both ends 3. Correct length 9.8cm and width 2cm to with in 2mm 4. Well fastened at the tips 5. Dart slashed and neatened 6. Pressed towards the C.F | 1  1  1  1  2  1 |  |  |
|  | **Sub Total** | **7** |  |  |
| **4** | **SHOULDER SEAM (MACHINE FELL SEAM)If not give zero** |  |  |  |
|  | 1. Straight stitchery of the first line 2. Straight stitchery of the second line close to the fold 3. Seam neatly tucked under 4. Correct width 6mm to within 2mm 5. Flat on the W.S and R.S 6. Seam pressed towards the C.B | 1  2  1  1  1  1 |  |  |
|  | **Sub Total** | **7** |  |  |
| **5** | **SIDE SEAM (Open neatened seam if not given; Zero)** |  |  |  |
|  | 1. Straight and firm stitchery 2. Seam pressed open and flat at arm hole and at the hem 3. Seam neatened 4. Correct size of the neatened seam turnings 1cm to within 2mm 5. Neatened Seam turnings even through out the length | 1  1  1  1  1 |  |  |
|  | **Sub Total** | **5** |  |  |
| **6** | **FACINGS** |  |  |  |
|  | 1. **JOINING THE FACINGS** 2. Front and back facing joined using open seam. *(If not give zero in this section).* 3. Seam with firm and straight stitchery 4. Both seam turnings trimmed to 1 cm 5. Seam pressed open and flat at the neck line and at the edge 6. **NEATENING OF THE FREE EDGE** 7. Free edge neatened by edge stitching 8. Smooth stitchery 9. Evenness of the edge stitching 10. Appropriate neatening allowance (0.5cm) | 1  1  1  1  1  1  1  1 |  |  |
|  | **Total** | **8** |  |  |
| 7 | **PREPARATION OF UNINTERFACED AND ATTACHMENT OF THE COLLAR** |  |  |  |
|  | **PREPARATION**   1. Collar Uninterfaced 2. Collar and under collar joined with smooth and curved stitchery 3. Well trimmed, knife edged and snipped   **ATTACHMENT**   1. Collar attached by sandwiching between the joined facing and garment 2. Joined with smooth and curved stitchery 3. Neckline evenly trimmed and snipped 4. Correct positioning of the collar 5. Flatness of the attached collar 6. Correct size (5cm to within 2mm) and shape of the attached collar | 1  1  11/2  1  1  1  1  1  1 |  |  |
|  | **Sub total** | **91/2** |  |  |
| 8 | **CONTINOUS WRAP OPENING** |  |  |  |
|  | 1. Correct size of the opening (6cm to within 2mm) 2. Sleeve binding attached with straight and firm stitchery 3. Tucked in completely concealing the raw edges 4. Held with hemming stitches 5. Binding pressed flat | 1  1  1  1  1 |  |  |
|  | **Sub total** | **5** |  |  |
| 9 | **UNDERARM SEAM (French seam if not give zero)** |  |  |  |
|  | 1. Straight and firm stitchery of the 1st line 2. Raw edges completely enclosed 3. Well knife –edged 4. Correct size 0.6cm to within 2mm 5. Evenness of the seam 6. Seam pressed towards the C.B | 1  1  1  1  1  1 |  |  |
|  | **Sub total** | **6** |  |  |
| 10 | **PREPARATION AND ATTACHMENT OF THE CUFF** |  |  |  |
|  | **PREPARATION**   1. Cuff joined with straight and firm stitchery 2. Seam allowance trimmed and the corner snipped 3. Well knife edged   **ATTACHMENT**   1. Cuff attached to the sleeve with firm, straight stitchery and trimmed 2. Held in place using hemming stitches 3. Correct size 4cm to within 2mm and shape of the cuff 4. Cuff pressed flat | 1  1  1  1  1  1  1 |  |  |
|  | **Sub total** | **7** |  |  |
| 11 | **ATTACHMENT OF THE SLEEVE** |  |  |  |
|  | 1. Sleeve attached with smoothly curved and straight stitchery 2. Raw edges and notches matching 3. Front sleeve joined to the front bodice and vice versa 4. Seam not trimmed and not neatened 5. Correct size of the seam allowance 6. Fullness evenly distributed at the crown 7. Underarm and side seam meeting at the armhole to within 2mm 8. Good hang of the sleeve | 1  1  1  1  1  1  1  1 |  |  |
|  | **Sub total** | **8** |  |  |
| 12 | **BUTTONHOLE STITCHES (if not give zero)** |  |  |  |
|  | 1. Good tension and evenness of the stitches 2. Fastened on and off 3. Single thread used 4. Both ends worked with square edge or round | 1  1  1  1 |  |  |
|  | **Sub total** | **4** |  |  |
| 13 | **HEM MANAGEMENT** |  |  |  |
|  | 1. Raw edges completely enclosed by double fold on the garment 2. Hem held using herring bone stitches (if not give zero from(b-f) 3. Good tension and evenness of the stitches 4. Fastened off and on 5. Hem flat and even in width 6. Correct size (1.5 cm to within 2mm) | 1  1  1  1  1  1 |  |  |
|  | **Sub total** | **6** |  |  |
|  | **G R A N D T O T A L** | **90/2** | **X/2** |  |