441/2

CLOTHING CONSTRUCTION

MARKING SCHEME

|  |  |  |  |
| --- | --- | --- | --- |
|  | Max score | Actual score | remarks |
| 1. **Presentation**  * Work well pressed(1) and folded(1/2) * Label firmly fixed (1) without concealing details (1/2 ) and on single fabric(1/2) * Pins/needles (1/2) tacking threads(1/2) and unnecessary threads (1/2) removed * Make up for the right half (1) | 1 ½  2 ½  1 ½  1 |  |  |
|  | **6 ½** |  |  |
| 1. **Cutting out**  * All five pieces cut out (5x1/2) * Smooth cutting of front bodice(1) * Smooth cutting of back bodice (1) and cut on straight grain(1) * Smooth cutting of back yoke(1) and cut on straight grain(1) * Smooth cutting of collar(1) and cut on straight grain(1) * Smooth cutting of back neck facing(1/2) cut on straight grain(1/2) | 2 ½  1  2  2  2  1 |  |  |
|  | **10 ½** |  |  |
| 1. **Making up** 2. Bust dart  * Correct length to within 2mm(1) * Correct width to within 2mm(1) * Tapering to a point (1) * Straight stitchery(1) * Threads secured (1) * Flat dart on R.S(1/2) and W.S(1/2) | 1  1  1  1  1  1 |  |  |
|  | **6** |  |  |
| 1. **Preparation of gathers**  * Two rows of gathering stitches above (1) and below (1/2) S.L * Gathers evenly distributed (2) * Gathering stitches not removed (1/2 x 2) | **2**  **2**  **1** |  |  |
|  | **5** |  |  |
| 1. **Attachment on the back yoke**   N.B If not overlaid seam give zero.  Overlaid seam   * Yoke folded on seam line (1) * Placed on F.L of the back bodice (1) * Straight stitchery (1) on the edge of the fold (1) * Overlaid turning facing upwards (1) * Even seam (1) * Flat yoke on the R.S (1) * Not neatened (1/2) not trimmed (1/2) * Matching notches (1/2) and edges (1/2) * Seam allowance 1.5cm from fitting line (1) to within 2mm. * Yokes CB and back bodice CB in flash (1) | **1**  **1**  **1**  **1**  **1**  **1**  **1**  **1**  **1** |  |  |
|  | **11** |  |  |
| 1. **Machine fell seam**   NB If not machine fell give zero.   * Straight stitchery of 1st row (1) * Fell well tucked under (1) and held down with straight stitchery (1) * Stitched close to the edge (1) * Even seam * Correct size (1) (0.4 – 0.8) * Flat seam on R.S (1) * Fell fixed towards the back of shoulder (1) * Thread secured (1) | **1**  **2**  **1**  **1**  **1**  **1**  **1**  **1** |  |  |
|  | **10** |  |  |
| 1. **Working of an open seam**   NB If not open seam give zero.   * Joining with straight stitchery (1) * Threads well secured (1) * Appropriate neatening (1/2 x 2) * Even seam (1) * Correct width 1cm on either side (1/2 x 2) * Seam opened (1) * Flat (1/2) and pressed (1/2) | **1**  **1**  **1**  **1**  **1**  **1**  **1** |  |  |
|  | **7** |  |  |
| 1. **Joining back and front facing**  * Correctly joined (1/2 x 2) with straight stitchery (1/2 x 2) * Free edge of facing correctly edge stitched (2) * Even (1) edge throughout * Flat seam (1) * Seam allowance trimmed (1) and pressed (1/2) open (1/2) | **2**  **2**  **1**  **1**  **2** |  |  |
|  | **7** |  |  |
| 1. **Preparation and attaching of collar**  * Correctly prepared (1) * Round (1) smooth (1) edges * Flat colour (1) * Correctly shaped (1) and size (1) * Correctly stitched (1) and attached * Correctly attached (1) and positioned (1) * Correctly neatened (1) with facing (1) * Facing lying flat (1) * Clipped seam (1) allowance | **1**  **2**  **1**  **2**  **1**  **2**  **2**  **1**  **1** |  |  |
|  | **13** |  |  |
| 1. **Understitching the facing**  * Correct understitching (1) * Stitches not seen on R.S (1) * Flat facing (1) * Seam allowance (1) * Threads secured (1) | **1**  **1**  **1**  **1**  **1** |  |  |
|  | **5** |  |  |
| 1. **Button hole**   NB if not button hole stitches award zero   * Correct positioning (1/2) and the length (1/2) of button hole * Button hole cut on straight grain (1) and worked with single thread (1) * Button hole stitches even (1/2) well distributed (1) * Round end worked with well distributed (1/2) overcastting (1/2) stitches * Square and complete with bar (1) worked with even (1/2) button hole stitches. * Row edges concealed by buttonhole stitches (1/2 x 2) | **1**  **1**  **1**  **1 ½**  **1**  **1 ½**  **1** |  |  |
|  | **8** |  |  |
|  | **90** |  |  |