**441/2**

**HOME SCIENCE**

**CLOTHING CONSTRUCTION**

**PAPER 2**

**PRACTICAL**

**MARCH, 2018**

**TIME: 21/2 HOURS**

**MOKASA JOINT EVALUATION EXAMINATION**

**Kenya Certificate of Secondary Education**

**441/2**

**Clothing and Textiles**

**(Practical)**

**JUNE, 2018**

**TIME: 21/2 HOURS**

A pattern of a girl’s dress is provided.

You are advised to study the paper patterns, sketches, instructions and the layout carefully before you begin the test.

**MATERIALS PROVIDED**

1. Pattern pieces

A – Dress Back

B - Dress front

C – Yoke

D – Front frill

E - Back frill

F - Front facing

G - Back facing

1. Plain weight cotton fabric 55cm long by 90 cm wide
2. Cotton sewing thread to match the fabric.
3. One large envelope

**THE TEST**

Using the materials provided cut out and make the **RIGHT HALF** of the child’s dress to show the following processes;

1. Cutting out. (15marks)
2. Joining the yoke to the front dress (12marks)
3. Making the shoulder seam using double stitched seam (8marks)
4. Making the side seam using open seam (7marks)
5. Making the inverted pleat on the front frill (5marks)
6. Joining the front and back frills using French seam (8marks)
7. Attach the frills to the dress using plain seam. **Don’t trim, don’t neaten** (9marks)
8. Joining the front to back facing and neatening the raw edge. (10marks)
9. Using the joined facings to neaten the neckline and front dress (7marks)
10. Presentation. (7 marks)

**At the end of the examination, firmly sew onto your work, on a single fabric, a label bearing your name and index number. Remove needles and pins from your work, fold your work neatly and place it in the envelope provided. Don’t put scraps of fabric in the envelope.**

90 cm

**LAYOUT (NOT DRAWN TO SCALE)**

**VIEWS**

**D**

55 cm

Selvedge

**F**

**C**

**E**

**G**

**B**

**A**

**FRONT VIEW**

**BACK VIEW**